Master index | Index for .

# Index for .

## Matlab files in this directory:

ListDir | 'ListDir': scan the structure of the directory tree (for dataview.m)
RUN_FIX | 'RUN_FIX': function for fixing velocity fields:
RUN_STLIN | 'RUN_STLIN': combine velocity fields for stereo PIV
calc_field | 'calc_field': defines fields (velocity, vort, div...) from civx data and calculate them
cell2tab | 'cell2tab': transform a Matlab cell in a character array suitable for display in a table
check_field_structure | 'check_field_structure': check the representation of fields by a Matlab structure
check_functions | 'check_functions': check the path and modification date for all the
civ | 'civ': function associated with the interface 'civ.fig' for PIV, spline interpolation and stereo PIV (patch)
civ_3D | 'civ_3D': function associated with the interface 'civ_3D.fig' for PIV in volume
close_fig | 'close_fig': function activated when a figure is closed
copyfields | 'copyfields' copy fields between two matlab structures
dataview | TEST 'dataview': function for scanning directories in a campaign (TEST)
datenum_uvmat | 'datenum_uvmat': like the Matlab function datenum.m but gives empty output instead of stopping for input error
delete_object | 'delete_object': delete a projection object, defined by its index in the Uvmat list or by its graphic handle
editxml | 'editxml': function for editing xml files using a xml schema (associated with the GUI editxml.fig)
find_field_indices | 'find_file_indices': group the variables of a nc-formated Matlab structure into 'fields' with common dimensions
geometry_calib | 'geometry_calib': performs geometric calibration from a set of reference points
get_field | 'get_field': display variables and attributes from a Netcdf file, and plot selected fields
get_plot_handles | 'get_plot_handles': list the handles of elements setting the plotting parameters in the uvmat interface
griddata_uvmat | 'griddata_uvmat': function griddata_uvmat(vec2_X,vec2_Y,vec2_U,vec_X,vec_Y,'linear')
hist_update | 'hist_update': update of a current global histogram by inclusion of a new field
imadoc2struct | 'imadoc2struct': reads the xml file for image documentation
interp2_uvmat | A matrix (npy,npx) to interpolate
keyboard_callback | 'keyboard_callback:' function activated when a key is pressed on the keyboard
mouse_down | 'mouse_down': function activated when the mouse button is pressed on a figure (callback for 'WindowButtonDownFcn'
mouse_motion | 'mouse_motion': permanently called by mouse motion over a figure (Callback for 'WindowButtonMotionFcn' of the figure)
mouse_up | 'mouse_up': function activated when the mouse button is released
msgbox_uvmat | 'msgbox_uvmat': associated with GUI msgbox_uvmat.fig to display message boxes, for error, warning or input calls
name2display | 'name2display': extracts the root name and field numbers from an input filename
name_generator | 'name_generator': creates a file name from a root name and indices.
nc2struct | 'nc2struct': transform a netcdf file in a corresponding matlab structure
nc2struct_toolbox | 'nc2struct_toolbox': transform a netcdf file in a corresponding matlab structure, USE OLD NETCDF LIBRARY
nomtype2pair | 'nomtype2pair': creates nomencalture for index pairs.
num2stra | 'num2stra': transform number to the corresponding character string depending on the nomenclature
parseXML | PARSEXML Convert XML file to a MATLAB structure. (from matlab help)
peaklock | 'peaklock': determines peacklocking errors from velocity histograms.
phys | 'phys': transforms image (px) to real world (phys) coordinates using geometric calibration parameters
phys_XYZ | 'phys_XYZ':transforms image (px) to real world (phys) coordinates using geometric calibration parameters
phys_polar | transform image coordinates (px) to physical coordinates
plot_field | 'plot_field': plot any field with the structure defined in the uvmat package
plot_object | 'plot_object': draws a projection object (points, line, plane...)
plot_text | 'plot_text': function for displaying the content of a Matlab structure in a figure
probe_calib | 'probe_calib': performs geometric calibration from a set of reference points
proj_field | 'proj_field': projects the field on a projection object
proj_grid | 'proj_grid': project fields with unstructured coordinantes on a regular grid
px | 'px': transform fields from physical coordinates (phys) to image (px) coordinates
px_XYZ | 'px_XYZ': transform phys coordinates to image coordinates (px)
pxcm_tsai | 'pxcm_tsai': find differentials of the Tsai calibration
raw2phys | 'raw2phys': transform raw signal to physical values using different calibrations laws
read_civxdata | 'read_civxdata': reads civx data from netcdf files
read_geometry_calib | 'read_geometry_calib': read data on the GUI geometry_calib
read_get_field | 'read_get_field': read the list of selected variables from the GUI get_field (SAME AS THE FIRST
read_get_field_old | 'read_get_field': read the list of selected variables from the GUI get_field (SAME AS THE FIRST
read_image | 'read_image': reads an image from a single file or a movie file
read_imatext | 'read_imatext': reads the .civ file for image documentation (obsolete)
read_plot_param | 'read_plot_param': read plotting parameters from the interface uvmat
read_set_object | 'read_set_object': read the data on the 'set_object' interface
read_xls | 'read_xls': function for reading and displaying Excel files
reinit | 'reinit': delete the personal parameter file 'uvmat_perso.mat'
series | 'series': master function associated to the GUI series.m for analysis field series
set_col_vec | 'set_col_vec': sets the color code for vectors depending on a scalar vec_C and parameters given by the struct colcode
set_grid | 'set_grid':produce grid for PIV with one or two images (stereo case)
set_object | 'set_object': GUI to edit a projection object
set_title | 'set_title': defines the 'TITLE' of a projection object
stra2num | 'stra2num': transform letters (a, b, c) or numerical strings ('1','2'..) to the corresponding numbers
struct2nc | 'struct2nc': create a netcdf file from a Matlab structure
struct2nc_toolbox | 'struct2nc_toolbox': create a netcdf file from a Matlab structure: use of netcdf toolbox
struct2xml | 'struct2xml': transform a matlab structure to a xml tree.
sub_field | 'sub_field': combines two input fields + mask for uvmat
update_menu | 'update_menu': find an input string in a menu, add it to the menu at the penultimate position if it does not exist
update_obj | 'update_obj': update the object graph representation and its projection field, record it in the uvmat interface
update_waitbar | 'update_waitbar': update the waitbar display, used for ACTION functions in the GUI 'series'
uvmat | 'uvmat': function associated with the GUI 'uvmat.fig' for images and data field visualization
warndlg_uvmat | 'warndlg_uvmat': display warning message (error, warning, confirmation) in a given figure
write_plot_param | 'write_plot_param': update the plotting parameters on the uvmat interface after a plotting operation

## Subsequent directories:

- @template_bad
- @xmltree
- FIELD_FCT
- IMA_TRANSFORM
- SCAL_TRANSFORM
- SERIES_FCT
- UVMAT_DOC
- VAR_TRANSFORM
- VEL_TRANSFORM